AT : Ceck the connection.  
AT+NAME : See default name  
AT+ADDR : see default address  
AT+VERSION : See version  
AT+UART : See baudrate  
AT+ROLE: See role of bt module(1=master/0=slave)  
AT+RESET : Reset and exit AT mode  
AT+ORGL : Restore factory settings  
AT+PSWD: see default password

AT+CMODE=0 allows the HC-05 to connect to any device  
AT+INQM=0,5,9 set inquiry to search for up to 5 devices for 9 seconds  
AT+INIT initiates the SPP profile. If SPP is already active you will get an error(17) which you can ignore.  
AT+INQ searches for other Bluetooth devices.  
  
  
AT+BIND=0021,13,00AD4E  
  
AT+PAIR=0021,13,00AD4E,20